|  |
| --- |
| **Vessel daily check** |
| Vessel ID:       | Date / time:       | Provider initials:       |
| Scheduled inspection | Description | Status | Comments |
| Completed |
| Vessel hull | Visual hull inspection | [ ]  Yes | [ ]  No |       |
| Bungs | [ ]  Yes | [ ]  No |       |
| Transom | [ ]  Yes | [ ]  No |       |
| Bimini secure | [ ]  Yes | [ ]  No |       |
| Anchor line secure | [ ]  Yes | [ ]  No |       |
| In-water leak test | [ ]  Yes | [ ]  No |       |
| Safety equipment and documentation | 4 PFD level 100 | [ ]  Yes | [ ]  No |       |
| Dan buoy | [ ]  Yes | [ ]  No |       |
| First aid kit | [ ]  Yes | [ ]  No |       |
| Fire extinguisher (visual) | [ ]  Yes | [ ]  No |       |
| Bucket with lanyard | [ ]  Yes | [ ]  No |       |
| Torches x 2 (test) | [ ]  Yes | [ ]  No |       |
| Two oars | [ ]  Yes | [ ]  No |       |
| Anchor, chain and line | [ ]  Yes | [ ]  No |       |
| Test of UHF radio | [ ]  Yes | [ ]  No |       |
| Mobile phone check (on battery life and waterproof case) | [ ]  Yes | [ ]  No |       |
| Laminated SOP and emergency contacts | [ ]  Yes | [ ]  No |       |
| Outboard and fuel | Outboard secure to transom and safety lanyard | [ ]  Yes | [ ]  No |       |
| Fuel tank visual, no leaks and fuel lines okay | [ ]  Yes | [ ]  No |       |
| Fuel tank secure to hull | [ ]  Yes | [ ]  No |       |
| Adequate fuel | [ ]  Yes | [ ]  No |       |
| Fuel line securely fitted to outboard | [ ]  Yes | [ ]  No |       |
| Propeller okay and secure | [ ]  Yes | [ ]  No |       |
| Engine run test and cooling water check | [ ]  Yes | [ ]  No |       |